seti@home

setHI@berkeley

The Berkeley SETI group (Erik Korpela, Dan Wertheimer;

undergrads Eric Heien, Shinae Park) and Carl Heiles

Technical Specifications:

• seti@home is centered on the 21-cm line;

BW = 2.5 MHz.

• Short line feed on Arecibo CH1, usually scans randomly through the sky at twice sidereal rate as CH2 tracks.

• Full coverage of most of Arecibo’s sky, ∼ 4 × 106 pixels of size 3 × 3 arcmin.

• 4.4 million spectra per year; 2 years accumulated already.

• 5 sec integration per spectrum, smearing over ∼ 2.5 arcmin.

• HP BW ≈ 5 arcmin.

3